# GStreamer source element name:
VIDEOSRC="icamerasrc"
#SPLASHSRC="filesrc location=/.../splash.png ! pngdec ! imagefreeze num-buffers=4 ! videoscale ! videoconvert"

# Output format, width, height, and frame rate:
FORMAT=YUY2
WIDTH=1280
HEIGHT=720
FRAMERATE=30/1

# Virtual video device name:
CARD_LABEL="Intel MIPI Camera"

# Extra options to pass to v4l2-relayd:
#EXTRA_OPTS=-d
